SHORT GUIDE FOR DEPLOYING


I have developed, debugged and preliminary tested the firmware on the PC running Ubuntu. The following is the steps for transferring the code to BBB and then compile, run the application on real Beagle-Bone Black.

1. First, I need to transfer the source code from my Ubuntu PC to BBB board. I assume that we have installed Debian Distribution on BBB. My BBB have IP address 10.10.1.144 and I will use default account in this guide.


Login name: debian

Password: temppwd

This is the directory structure of project on my Ubuntu PC




I will use the scp command to copy code to BBB



1. After transferring the source code to the BBB. It is ready to deploy the application on the real hardware. Again, I will use the putty from my Windows PC to do tasks

Showing the source code on the BBB



1. As of now, I have used cmake to re-compile the source code on the BBB. So there are some dependencies we need to install on the BBB: cmake, boost library (for some utilities)

The followings were the commands to install

debian@beaglebone:$ sudo apt-get update

debian@beaglebone:$ sudo apt-get install cmake

debian@beaglebone:$ sudo apt-get install cmake

debian@beaglebone:$ sudo apt-get install libboost-dev

1. When all dependencies were installed, we are ready to compile our project


NOTE:

Before compiling the source code, you must update IP address and port settings on source code matching with current settings of your testing environment.


+ Open file main.cpp in “master” directory and update IP address and port information to permit it connects to submaster application

+ Open file main.cpp in “submaster” directory and update IP address setting to IP address of submaster itself.


* Make sure we were in the root directory of project
* Make new directory for building progress, for example “build”




* Move to just-created “build” directory and run “cmake ..” command. If everything was right, we will have similar screen as below




* Next, run “make” command and wait for a while (2 or 3 minutes) before compiling progress to finish
* Again, If everything was right, we will have similar screen as below



The compile will create 2 sub-directories under “build” directory. The one was used to store binary file for master application, the other was used to store binary file for submaster application.





Now, we have binary files for both master and submaster applications. You can test them with the simulator and real external serial devices.

JSON FORMAT OF SETTINGS

{

"version": "1.0.0",

"self\_id": 0,

"units": [

{

"unit\_type": "master",

"unit\_id": 0,

"unit\_ipaddr": "192.168.1.1"

},

{

"unit\_type": "slave",

"unit\_id": 1,

"unit\_ipaddr": "192.168.1.2"

},

.

.

.

{

"unit\_type": "submaster",

"unit\_id": 9,

"unit\_ipaddr": "192.168.1.10"

}

]

}

The application on each BBB should have its own settings.json file was on the same directory with binary file of the application

+ The "self\_id" element in JSON string used to identify the unit

+ The settings.json file for Master should have "self\_id" assigned to 0

+ The settings.json file for Submaster should have "self\_id" assigned to 9


+ The settings.json file for Slave should have "self\_id" assigned to 1 – 8

+ The "units" array stores all information of all units in details and this array should be the same on all BBBs

WEB SETUP

1. Install node.js and Express.js

Latest debian distribution on Beagle Bone Black have pre-installed node.js and Node Package Manager (npm) as picture below:




But, this is not the latest version of node.js as well as npm component

So, we need to run some commands to update node.js and npm to latest versions.


* First, run this command

curl -sL https://deb.nodesource.com/setup\_6.x | sudo -E bash –




* Next, run

sudo apt-get install -y nodejs



After installation process was done, both node.js and npm were updated to latest version




When you go at here, you are ready to deploy the web application. The production web application should be self-contained and have integrated all required components and dependencies (included Express.js)

However, it is better for you know the process creating the Express.js web application. The following sections will detail the steps that I have done.

1. Install Express Application Generator


This tool was used to create skeleton Express.js web application. So run this command to install Express Application Generator for system global

* sudo npm install express-generator –g




* Next, go to the directory that you want the new web application was located. Now, I will use home directory of current account - /home/debian.

Run command cd /home/debian




* Next, we will use application generator to create web application named web-app at /home/debian.

Run command express -e -c less -f web-app




We will see the screen when the command was completed



As the hints on the screen. Next step should be go to new created directory (web-app) and run command ‘nmp install)

* Go to web-app directory and run npm install

When the command was completed you will see the screen like this








* At that time, you can start web application. But with my experience, it looks like the 3000 port have used by some other application, I don’t know which application now. So we need to change the default port from 3000 to 3030 for example.
* Go to bin directory and open file www as follow




And change 3000 value to 3030 as follow




Save and exit

* Go back to parent of the bin (it is web-app directory) and start the web with command node ./bin/www



Now the web have started and you can access to the skeleton application with your browser





* At that time, we have setup the web application. The final steps were to pull 3 files from GIT and copy them into the web application

Copy the file index.js from web-app/routes on GIT and paste it on web-app/route on the BBB.

Copy files index1.ejs, index2.ejs from web-app/views on GIT and paste them on web-app/views on the BBB.

Stop the web and re-run it. And now you can access two web pages for our system.





I will continue with data-binding and more features !!!